RFQ 1681 – Kerr House Sump Replacement

Q&A

1. Are these needing to be priced with 100-foot cables less the control boxes? Yes, 100 ft cable and no control boxes are needed.
2. Confirm the required duty point (head and flow).  We can estimate what is required based on the included GR curve but will need the duty eventually. It needs to meet or exceed the GR curve @ 75’ of head, approx.. 1050 GPM
3. Can you please specify the liquid being pumped? Water